|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **LaMAS BASE MODEL PRICE LIST** | | | | | |
| **LaMAS CONTRACT # 4400017445** | | | | | |
| **ROSENBAUER AMERICA, LLC** | | | | | |
|  | | | |  | 10/18/2021 |
| For Fire Fighting Vehicles (Pumpers, Tankers, Aerials, Rescues, Specialty Apparatus) | | | |  |  |
|  | **GSA Pricing** | **LaMAS** | **LaMAS** | **LaMAS** | **LaMAS** |
|  |  | **1 Unit** | **2-5 Units** | **6-10 Units** | **11+ Units** |
| ***Custom Pumper*** RBA1131-1L | $671,257.55 | $666,223.12 | $664,557.56 | $662,892.01 | $661,226.49 |
|  |  |  |  |  |  |
| Rosenbauer custom cab chassis, full height and full depth body compartments, minimum 750gpm water pump, 500-gallon water tank, ground ladder storage and hose storage. Meets NFPA 1901-2016 and EPA 17 standards. |  |  |  |  |  |
| ***100+ Custom Aerial Ladder***  RBA1103-2L | $1,071,037.42 | $1,063,004.64 | $1,060,347.13 | $1,057,689.62 | $1,055,032.18 |
|  |  |  |  |  |  |
| Rosenbauer custom cab chassis, 4 section steel aerial ladder, minimum 1250gpm water pump, 300-gallon water tank, 1000gpm aerial monitor, 500lb tip load and 2 station intercom system. Meets NFPA 1901-2016 and EPA 17 standards. |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| ***Light Rescue*** RBA1341 | $134,670.10 | $133,660.07 | $133,325.92 | $132,991.77 | $132,657.62 |
| Ford F550 4WD Chassis, 19,500 GVWR, Rosenbauer Formed Aluminum 12' rescue body, LED Warning Light Package, LED Compartment Lighting Package, Coffin Box Roof Storage, Breathing Air System, 5kW Gas Generator. Meets NFPA 1901-09 and EPA 10 Standards. |  |  |  |  |  |
|  |  |  |  |  |  |
| ***Rescue, 2-Door, Special*** RBA1245X | $396,147.77 | $393,176.66 | $392,193.71 | $391,210.77 | $390,227.83 |
| Two-door chassis, 47,000 GVWR chassis, 450 HP, Automatic transmission, A/C, Rosenbauer aluminum rescue body, breathing air system, generator, Roll-up doors, LED Warning light package. Many additional options available. Meets NFPA 1901-09. |  |  |  |  |  |
|  |  |  |  |  |  |
| ***Custom 4-Door Heavy Rescue*** RBA1247 | $418,991.65 | $415,849.21 | $414,809.59 | $413,769.96 | $412,730.34 |
| Custom Chassis, 47,000 GVRW chassis, 450 HP, Automatic transmission, A/C, Rosenbauer aluminum rescue body, Roll-up doors, 25kW PTO Generator, LED Warning light package. Meets NFPA 1901-09 and EPA 10 Standards. |  |  |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
| **LaMAS BASE MODEL PRICE LIST** | | | | | |
| **LaMAS CONTRACT # 4400017445** | | | | | |
| **ROSENBAUER AMERICA, LLC** | | | | | |
|  | | | |  | 7/1/2018 |
| For Fire Fighting Vehicles (Pumpers, Tankers, Aerials, Rescues, Specialty Apparatus) | | | |  |  |
|  | **GSA Pricing** | **LaMAS** | **LaMAS** | **LaMAS** | **LaMAS** |
|  |  | **1 Unit** | **2-5 Units** | **6-10 Units** | **11+ Units** |
| ***Rapid Intervention Vehicle C2*** RBA1110 | $195,861.89 | $194,392.93 | $193,906.95 | $193,420.97 | $192,934.99 |
| Rosenbauer C2 Rapid Intervention Vehicle (RIV), Aircraft Rescue/Firfighting Vehicle, Dual agent, Ford F550 Super Duty, 4x4, 2-Door chassis, 19,500 GVWR, 6.4L 325 Hp.V8 Diesel engine, Automatic Transmission, Aluminum Body, Cross-mount 250 gpm pump & roll, foam system, 300 gallon poly water tank w/lifetime warranty, 40 gallon foam tank, 500 # Dry Chem., Roll-up doors, tilt table tested, In-cab pump & turret controls, Complies with NFPA 414 & FFA 150/5220-10D. |  |  |  |  |  |
|  |  |  |  |  |  |
| ***Wildland Urban Interface Pumper*** RBA0619 | $227,175.25 | $225,471.44 | $224,907.77 | $224,344.09 | $223,780.41 |
| International 4x4 two-door chassis, 230 Hp, Automatic transmission, Extruded aluminum body & sub-frame, Rosenbauer NH1000 GPM pump& roll, High pressure foam proportioning system, Front bumper turret w/  1.5" electric valve, 750 gal. water, 30 gal. foam, 24" full depth / full height side compartments. Meets current NFPA standards. |  |  |  |  |  |
|  |  |  |  |  |  |
| ***85' Platform*** RBA1405 | $855,255.42 | $848,841.00 | $846,718.90 | $844,596.80 | $842,474.69 |
| Custom Chassis, 85' aerial platform, 83,000 GVWR, 500 Hp Diesel Engine, Automatic Transmission, Aluminum Body, 1500 GPM, 400 Gal. Tank, Outriggers, Rosenbauer SMART aerial. Meets NFPA 1901-09 and EPA 10 Standards. |  |  |  |  |  |
|  |  |  |  |  |  |
| ***101' Aerial Platform*** RBA1179 | $947,246.91 | $940,142.56 | $937,792.20 | $935,441.85 | $933,091.49 |
|  |  |  |  |  |  |
| Custom 4-Door Chassis, 81,000 GVWR, A/C, 2000 GPM Pump, 500 Gallon Poly Water Tank  with Lifetime Warranty, Aluminum Aerial Body, Heavy Duty 101’ Cobra Smart Aerial Platform Device, 1000 Lb. Tip Load at any angle flowing water, 1500 GPM aerial monitor, two station aerial intercom system. Meets NFPA 1901-09. |  |  |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
| **LaMAS BASE MODEL PRICE LIST** | | | | | |
| **LaMAS CONTRACT # 4400017445** | | | | | |
| **ROSENBAUER AMERICA, LLC** | | | | | |
|  | | | |  | 7/1/2018 |
| For Fire Fighting Vehicles (Pumpers, Tankers, Aerials, Rescues, Specialty Apparatus) | | | |  |  |
|  | **GSA Pricing** | **LaMAS** | **LaMAS** | **LaMAS** | **LaMAS** |
|  |  | **1 Unit** | **2-5 Units** | **6-10 Units** | **11+ Units** |
| ***Panther ARFF 1500 4X4 WIDE*** RBA1112 | $551,141.72 | $547,008.16 | $545,640.64 | $544,273.12 | $542,905.60 |
| ARFF Panther, Detroit Series 60 665 HP, Twin Disc transmission, High mobility on/off road suspension, Aluminum body, Centrifugal high performance pump, Fully automatic foam proportioning system, Roof turret, Bumper turret, Quick attack lines, 1500 gal. water, 200 gal. foam, roll-up doors. Meets NFPA 414, FAA 150/5220-10D and EPA 07 Standards. |  |  |  |  |  |
|  |  |  |  |  |  |
| ***Panther ARFF 3000 6x6*** RBA1114 | $588,365.93 | $583,953.19 | $582,493.31 | $581,033.43 | $579,573.54 |
| ARFF Panther, Detroit Series 60 665 HP, Twin Disc transmission, High mobility on/off road suspension, Aluminum body, Centrifugal high performance pump, Fully automatic foam proportioning system, Roof turret, Bumper turret, (2) Quick attack lines, 3000 gal. water, 400 gal. foam, Roll-up doors. Meets NFPA 414, FAA 150/5220-10D and EPA 07 Standards. |  |  |  |  |  |