|  |
| --- |
| Attachment B - Base Model PricingFerrara Fire Apparatus LaMAS Contract 4400027889 |
| **Product Number Product Description LaMas Price** |
| Cinder-77HDRML-22 | Cinder HD77 Rear Mount Ladder: NFPA 1901 compliant, Ferrara Cinder custom chassis, Cummins L9 450 hp engine, automatic transmission, medium 4-door (MFD) tilt flat roof cab, seating for six, 400 gallon tank, 1500 GPM midship pump, heavy duty extruded aluminum EZ Stack body | $852,771.81 |
| Cinder-HDRescueWA-22 | Cinder HD Walk-Around Rescue: NFPA 1901 compliant, Ferrara Cinder 4x2 custom chassis, medium 4-door (MFD) tilt flat roof cab, seating for six, Cummins L9 350 hp engine, automatic transmission, 136" cab-to-axle rescue body with extruded aluminum construction, roll up compartment. | $394,546.52 |
| Cinder-HDRESCUEWI-22 | Cinder HD Walk-In Rescue: NFPA 1901 compliant, Ferrara Cinder 4x2 custom chassis, medium 4-door (MFD) tilt flat roof cab, seating for six, Cummins L9 350 diesel, automatic transmission, 136" cab-to-axle WALK IN rescue body with extruded aluminum construction, roll up compartment doors, Whelen LED warning lights and siren and additional options. | $441,707.97 |
| Cinder-Pumper-22 | Cinder Extruded Side Mount Pumper: NFPA 1901 compliant, Ferrara Cinder 4x2 custom chassis, seating for six, Cummins L9 350 hp engine, automatic transmission, medium 4-door (MFD) tilt flat roof cab, 1000 gallon poly tank, 1500 GPM pump, heavy duty extruded aluminum body with left high sides and additional options. | $475,830.73 |
| Cinder-Tanker3000-16 | Cinder 3000 Gallon Tanker: NFPA 1901 compliant, Ferrara Cinder 4x2 custom chassis, seating for six, Cummins L9 350 hp engine, automatic transmission, medium 4-door (MFD) tilt flat roof cab, 3000 gallon poly tank, 1250 GPM pump, heavy duty extruded aluminum body with left high sides and additional options. | $548,021.92 |
| F5502D-LDRescue-22 | 2-Door F550 LD Walk-Around Rescue: NFPA 1901 compliant, Ford F500 2-door 4x2 chassis, diesel engine, automatic transmission, 84" cab-to-axle rescue body with extruded aluminum construction, Whelen warning lights and siren and additional options. | $162,573.36 |
| F5504D-LDRESCUE-22 | 4-Door F550 LD Walk-Around Rescue: NFPA 1901 compliant, Ford F550 4-door 4x2 chassis, diesel engine, automatic transmission, 84" cab-to-axle rescue body with extruded aluminum construction, Whelen warning lights and siren and additional options. | $168,994.46 |

|  |
| --- |
| Attachment B - Base Model PricingFerrara Fire Apparatus LaMAS Contract 4400027889 |
| **Product Number Product Description LaMas Price** |
| F550EC-LDRESCUE-22 | Extra Cab F550 LD Walk-Around Rescue: NFPA 1901 compliant, Ford F550 extra cab 4x2 chassis, diesel engine, automatic transmission, 84" cab-to-axle rescue body with extruded aluminum construction, Whelen warning lights and siren and additional options. | $164,926.35 |
| Frtlnr2D-MDRescueWA-22 | 2-Door Freightliner MD Walk-Around Rescue: NFPA 1901 compliant, 2-door Freightliner 4x2 custom chassis, Cummins L9 350 hp engine, automatic transmission, 108" cab-to-axle rescue body with extruded aluminum construction, roll up compartment doors, Whelen LED warning lights and siren. | $201,922.46 |
| Frtlnr2D-MDRESCUEWI-22 | 2-Door Freightliner MD Walk-In Rescue: NFPA 1901 compliant, 2-door Freightliner 4x2 custom chassis, Cummins L9 350 hp engine, automatic transmission, 108" cab-to-axle WALK-IN rescue body with extruded aluminum construction, roll up compartment doors, Whelen LED warning lights and siren and additional options. | $219,230.69 |
| Frtlnr2D-Pumper-22 | 2-Door Freightliner Extruded Side Mount Pumper: NFPA 1901 compliant, 2-door Freightliner M2 4x2 chassis, Cummins L9 350 hp engine, automatic transmission, 1000 gallon poly tank, 1250 GPM pump, heavy duty extruded aluminum body with left high side compartments, 14'/24'/10' ladders, two 6" x 10' suction hoses. | $290,966.69 |
| Frtlnr2D-Tanker3000-22 | 2-Door Freightliner 3000 Gallon Tanker: NFPA 1901 compliant, 2-door Freightliner chassis, Cummins L9 350 hp engine, automatic transmission, 3000 gallon poly tank, 1250 GPM pump, heavy duty extruded aluminum body with left high side compartments, 14'/24'/10' ladders, two 6" x 10' suction hoses. | $264,015.46 |
| Frtlnr4D-MDRESCUEWA-22 | 4-Door Freightliner MD Walk-Around Rescue: NFPA 1901 compliant, 4-door Freightliner 4x2 custom chassis, Cummins L9 350 hp engine, automatic transmission, 108" cab-to-axle rescue body with extruded aluminum construction, roll up compartment doors, Whelen LED warning lights and siren and additional options. | $215,930.78 |
| Frtlnr4D-MDRESCUEWI-22 | 4-Door Freightliner MD Walk-In Rescue: NFPA 1901 compliant, 4-door Freightliner 4x2 custom chassis, Cummins L9 350 hp engine, automatic transmission, 108" cab-to-axle WALK-IN rescue body with extruded aluminum construction, roll up compartment doors, Whelen LED warning lights and siren and additional options. | $244,833.13 |

|  |
| --- |
| Attachment B - Base Model PricingFerrara Fire Apparatus LaMAS Contract 4400027889 |
| **Product Number Product Description LaMas Price** |
| Frtlnr4D-PUMPER-22 | 4-Door Freightliner Extruded Side Mount Pumper: NFPA 1901 compliant, 4-door Freightliner M2 4x2 chassis, Cummins L9 350 hp engine, automatic transmission, 1000 gallon poly tank, 1250 GPM pump, heavy duty extruded aluminum body with left high side compartments, 14'/24'/10' ladders, two 6" x 10' hard suction with strainer. | $306,386.02 |
| Frtlnr4D-Tanker3000-22 | 4-Door Freightliner 3000 Gallon Tanker: NFPA 1901 compliant, 4-door Freightliner chassis, Cummins L9 350 hp engine, automatic transmission, 3000 gallon poly tank, 1250 GPM pump, heavy duty extruded aluminum body with left high side compartments, 14'/24'/10' ladders, two 6" x 10' hard suction with strainer. | $279,820.86 |
| Igniter-HDRESCUEWA-22 | Igniter HD Walk-Around Rescue: NFPA 1901 compliant, Ferrara Igniter 4x2 custom chassis, medium 4-door (MFD) tilt flat roof cab, seating for six, Cummins L9 350 hp engine, automatic transmission, 136" cab-to-axle rescue body with extruded aluminum construction, roll up compartment doors, Whelen LED warning lights and siren and additional options. | $410,942.39 |
| Igniter-HDRESCUEWI-22 | Igniter HD Walk-In Rescue: NFPA 1901 compliant, Ferrara Igniter 4x2 custom chassis, medium 4-door (MFD) tilt flat roof cab, seating for six, Cummins L9 350 hp engine, automatic transmission, 136" cab-to-axle WALK IN rescue body with extruded aluminum construction, roll up compartment doors, Whelen LED warning lights and siren and additional options. | $458,103.84 |
| Igniter-PUMPER-22 | Igniter Extruded Side Mount Pumper: NFPA 1901 compliant, Ferrara Igniter 4x2 custom chassis, seating for six, Cummins L9 350 hp engine, automatic transmission, medium 4-door (MFD) tilt flat roof cab, 1000 gallon poly tank, 1500 GPM pump, heavy duty extruded aluminum body with left high side compartments, 14'/24'/10' ladders, two 6" x 10' hard suction with strainer. | $484,883.26 |
| Igniter-Tanker3000-22 | Igniter 3000 Gallon Tanker: NFPA 1901 compliant, Ferrara Igniter 4x2 custom chassis, seating for six, Cummins L9 350 hp engine, automatic transmission, medium 4-door (MFD) tilt flat roof cab, 3000 gallon poly tank, 1250 GPM pump, heavy duty extruded aluminum body with left high side compartments, 14'/24'/10' ladders, two 6" x 10' hardsuction with strainer. | $564,417.79 |

|  |
| --- |
| Attachment B - Base Model PricingFerrara Fire Apparatus LaMAS Contract 4400027889 |
| **Product Number Product Description LaMas Price** |
| Inferno-100HDMMP-22 | Inferno HD-100 MMP: NFPA 1901 compliant, Ferrara Inferno custom chassis, Cummins X12 400 hp engine, automatic transmission, medium 4-door (MFD) tilt flat roof cab, seating for six, 400 gallon tank, 1500 GPM midship pump, heavy duty extruded aluminum EZ Stack body, 100' mid mounted heavy duty aerial platform, electric monitor, 2- way intercom, tip controls for monitor, NFPA 115' ground ladders, eight pike poles and additional options. | $1,327,175.74 |
| Inferno-100HDRMP-22 | Inferno HD-100 RMP: NFPA 1901 compliant, Ferrara Inferno custom chassis, Cummins X12 400 hp engine, automatic transmission, medium 4-door (MFD) tilt flat roof cab, seating for six, 400 gallon tank, 1500 GPM midship pump, heavy duty extruded aluminum EZ Stack body, 100' rear mounted heavy duty aerial platform, electric monitor, 2- way intercom, tip controls for monitor, NFPA 115' ground ladders, eight pike poles and additional options. | $1,137,472.42 |
| Inferno-107HDRML-22 | Inferno HD107 Rear Mount Ladder: NFPA 1901 compliant, Ferrara Inferno custom chassis, Cummins X12 400 hp engine, automatic transmission, medium 4-door (MFD) tilt flat roof cab, seating for six, 400 gallon tank, 1500 GPM midship pump, heavy duty extruded aluminum EZ Stack body, 107' rear mounted heavy duty aerial ladder, electric monitor, 2-way intercom, tip controls for monitor, NFPA 115' ground ladders, eight pike poles and additional options. | $1,063,141.52 |
| Inferno-77HDRML-22 | Inferno HD77 Rear Mount Ladder: NFPA 1901 compliant, Ferrara Inferno custom chassis, Cummins X12 400 hp engine, automatic transmission, medium 4-door (MFD) tilt flat roof cab, seating for six, 400 gallon tank, 1500 GPM midship pump, heavy duty extruded aluminum EZ Stack body, 77' rear mounted heavy duty aerial ladder, electric monitor, 2-way intercom, tip controls for monitor, NFPA 115' ground ladders, eight pike poles and additional options. | $859,495.05 |
| Inferno-HDRescueWA-22 | Inferno HD Walk-Around Rescue: NFPA 1901 compliant, Ferarra Inferno 4x2 custom chassis, medium 4-door (MFD) tilt flat roof cab, seating for six, Cummins X12 400 hp engine, automatic transmission, 136" cab-to-axle rescue body with extruded aluminum construction, roll up compartment doors. | $436,937.81 |

|  |
| --- |
| Attachment B - Base Model PricingFerrara Fire Apparatus LaMAS Contract 4400027889 |
| **Product Number Product Description LaMas Price** |
| Inferno-HDRESCUEWI-22 | Inferno HD Walk-In Rescue: NFPA 1901 compliant, Ferrara Inferno 4x2 custom chassis, medium 4-door (MFD) tilt flat roof cab, seating for six, Cummins X12 400 hp engine, automatic transmission, 136" cab-to-axle WALK IN rescue body with extruded aluminum construction, roll up compartment doors, Whelen LED warning lights and siren and additional options. | $490,842.26 |
| Inferno-PUMPER-22 | Inferno Extruded Side Mount Pumper: NFPA 1901 compliant, Ferrara Inferno 4x2 custom chassis, seating for six, Cummins X12 400 hp engine, automatic transmission, medium 4-door (MFD) tilt flat roof cab, 1000 gallon poly tank, 1500 GPM pump, heavy duty extruded aluminum body with left high side compartments, 14'/24'/10' ladders,two 6" x 10' hard suction with strainer. | $518,004.80 |
| Inferno-SuperPumper-22 | Extruded Side Mount Pumper: NFPA 1901 compliant, Ferrara Inferno 4x2 custom chassis, Cummins X15 605 hp engine, automatic transmission, raised roof cab, 1000 gallon poly tank, US Pumps 5250 GPM pump, Accumax 3300 foam system, 6” Rear discharges. | $1,312,363.67 |
| Inferno-Tanker3000-22 | Inferno 3000 Gallon Tanker: NFPA 1901 compliant, Ferrara Inferno 4x2 custom chassis, seating for six, Cummins X12 400 hp engine, automatic transmission, medium 4-door (MFD) tilt flat roof cab, 3000 gallon poly tank, 1250 GPM pump, heavy duty extruded aluminum body. | $589,772.39 |
| Ingiter-77HDRML-22 | Igniter HD77 Rear Mount Ladder: NFPA 1901 compliant, Ferrara Igniter custom chassis, Cummins L9 450 hp engine, automatic transmission, medium 4-door (MFD) tilt flat roof cab, seating for six, 400 gallon tank, 1500 GPM midship pump, heavy duty extruded aluminum EZ Stack body, 77'. | $834,140.45 |